Topline range

low temperatures :
• LT series: down to–60°C
high speeds:
• HV series: up to 700,000 N.Dm
This range benefits from all SNR's latest technological innovations :
• optimized internal geometry, with closer tolerances and greater precision for the HV series
• heat treatment adapted to the service conditions
• possibility of two types of sealing:
• by fluoroelastomer seal for the FT and HT series
• by shield

| back --> |  |