• induction heating appliances: 3 models available, to allow the clean and totally safe fitting of bearings from 210 to 740 mm inside diameter (bore). With pivoting arm, two modes of operation: temperature or time, automatic demagnetization at end of cycle.
But other models also exist, so don't hesitate to contact us if none of the above 3 models suits your needs!
• mallets and mounting paste to facilitate the installation of your bearings

|  | back --> |