Lubsolid

What is an SNR LubSolid bearing?
It is a bearing consisting of a porous polymer matrix containing a large quantity of oil that occupies the majority of the free volume of the bearing. Compression of the matrix ensures permanent lubrication of the ball-ring contact surface.
LubSolid can be adapted to all types of bearings (from 5mm bore to 450 mm outside diameter), with or without cage, with or without seal, complete or partial filling.

|  |  |  |  |  | back--> |