Sensor

SENSOR LINE ENCODER
For more than 10 years now SNR has maintained its research efforts in the field of mecatronics.
Today it can propose an active device for the high-resolution measurement of angular displacements:
• 1,024 points in one revolution (4,096 transitions), that is to say an angular resolution finer than 1/10°of a degree of angle.
• the direction of rotation
• an additional "Revolution Start" signal for counting the number of revolutions
• analogue temperature measurement

|  |  |  |  |  |  | back --> |