double-row spherical roller bearings

Thanks to this optimization, the service life of SNR double-row spherical roller bearings compare very favourably with the products available on the market. As SNR has opted to conserve the universally recognized method of calculating bearing life, you will have no difficulty in making the comparison!

|  |  |  |  |  |  |  | back --> |

La gamme SNR comporte 4 séries :
• Série E pour toutes les températures ne dépassant pas 150°C
• Série EA pour des températures au-delà de 150°C
• Série EM pour applications difficiles : hautes vitesses, chocs, pollution avec une cage massive
• Série EF 800 pour applications vibrantes : cribles, concasseurs, broyeurs…avec une cage monobloc usinée dans la masse